                                                  HOIST INSPECTION CHECKLIST

                                             Company Name________________________________

Date_____________________

HOIST#









MANUFACTURER







CRANE TYPE








CAPACITY








DEPARTMENT



















STATUS










OK

NEEDS














ATTENTION

1.
FUNCTIONAL MECHANISMS









1.
PUSH BUTTON PENDANT











2.
RETURN SPRING












3.
SPEED STRAPS












4.
UPPER LIMIT SWITCH












5.
HOIST BRAKE













6.
DIRECTIONAL CONTROLS











7.
WIRING-CONTROL & FITTINGS









2.
HOOKS

1.
ANY DEFORMATIONOR CRACKS










2.
HAS THROAT OPENING INCREASED MORE THAN



15% OVER NORMAL SIZE











3.
IS HOOK TWISTED MORE THAN 10%









4.
LOCKING DOGS ON HOOK









3.
HOISTING CABLE AND REEVING

1.
BROKEN WIRES












2.
CRUSHED












3.
STRETCHED












4.
TWISTED












5.
KINKED












6.
EXCESSIVE WEAR











7.
IS CABLE FOLLOWING DRUM GROOVES







4.
HOISTING CHAIN AND CONNECTIONS


1.
EXCESSIVE WEAR











2.
TWIST














3.
DISTORTED LINKS












4. 
STRETCHES BEYOND MFG. RECOMMENDATIONS







5.
GENERAL


1.
TAG & CAPACITY VISIBLE & LEGIBLE








2.
MOUNTING HARDWARE, IE, TIGHTNESS PRESENT







3.
TRACK/ROLLER












4.
APPROPRIATE LIBRICATION











5.
APPROPRIATE WARNING LABELS










6.
WARNING SIGNS IN PLACE











7.
CAPACITY RATINGS
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