Grounding Trucks and Equipment 
Should uninsulated parts of an aerial truck or stringing equipment contact energized parts, a low impedance connection to ground is needed to help minimize exposure to hazardous voltage. A truck ground attached to a system neutral or a ground rod with low impedance will provide a “tripping ground” to operate breakers, fuses, and other protective devices. Grounds shall be:
· Properly sized to match the electrical systems characteristics such as maximum fault currents, system protection schemes, and other engineering factors. 
· At least #2AWG and tested to ensure their current carrying capacity and mechanical strength match your systems requirements. 
· Completely removed from reels or coils when in use and applied to the system neutral or equivalent ground with a live line tool. 
[bookmark: _GoBack]No one shall contact grounded trucks or equipment while they are bonded to a system neutral or equivalent ground.  Grounding mats or other voltage rated rubber materials can be placed around the grounded equipment to help provide an equipotential zone for ground personnel. 
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