Substation Work
[bookmark: _GoBack]Any job around or inside a substation requires a clear understanding of the potential hazards. Verbal communication with the owner or operator of the substation should take place before entering a substation. Wear PPE required by your employer for entry such as FR clothing, face shield, etc  A visual inspection of the site shall be performed before entering the fence. Look for gaps in the fence or gates that could allow animals or un-authorized people to enter. Verify that each section of fence and all gates have grounds intact. Warning or danger signs shall be legible and visible from all sides. Information identifying the owner of the site, contact information, and address shall be posted on the main entrance. Continue a visual inspection of the substation components as you enter looking for leaking transformers, regulators, breakers, damaged or missing grounds, bird nests, or evidence of failed or damaged equipment. Gates used for entry shall be closed behind the entrant to deter animals and unqualified people from entering. Vegetation should be controlled around and inside the fence. Be aware that live parts may be much closer to the ground and have different minimum approach distances for higher voltages. Breakers, tap changers, regulators, switches, and any other distribution or transmission equipment shall be inspected for damage before operating.
