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A necessary device in our utility systems can prove dangerous to workers if they are not aware of hazards associated with them. When working with arrestors;
· Can work be done de-energized?
· Is the arrestor rated for the system voltage?  
· Connect the ground first, phase last. Reverse order when removing from service.
· Install the phase connection with a live line tool.
· Proper PPE worn (face shield, gloves, sleeves, safety glasses).
· Distance yourself from the arrestor.
· Use of energy source control devices?
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